
# Version 5.0.0
Standard allPIXAevo 16K CoaXPress
## Component Versions
|      Variant      |         Version         |
|   ------------    |      -------------      |
| Bitstream         |          21.0.0         |
| Application/XML   |          11.1.1         |
| Bootfile          |          11.1.0         |
| Feature Reference |          11.1.1         |
| Gamma    	        |      KaxGamma03_10      |


## Notes




## Changes and new Features

* Support multi ROI (Region1-4)
* Added MultRegionMerge feature to enable single virtual region **RegionStream0**
* Allow user set loading even if flat field correction calibration mode is active
* Support new feature InfoBlockTriggerSource to trigger the first line info block by an IO
* Refactoring on Gain Control (Application supports 12-Ch-BV mono)
* The gain control width and offset is limited to certain multiples
  * If the gain control is outside an ROI the start of the ROI is expected to be precise.
* Changed EachLineInfoBlock to the used 8 pixels 2 markers
* Adaption of log level of some camera loggings
* Added support for new power board 921
* Power file upload can be done outside maintenance mode (if supported)
* Extended the power board version string in the DeviceVersion feature
* Support Digital IO User Output
* Common sensor control (anactrl) for all sensors.
* Introduced sensor/acquisition locking (Package must match for camera)
* New desegmentation IP


## Bug Fixes

* Fixed the bug to download DSNU/PRNU files to the PC when the description was changed
* Fixed the bug to set image height correctly during internal reference capturing
* Fixed the bug in preparing the parameters for internal reference capturing.
* Fix for FlatFieldCorrectionCalibrationMode
  * Changing between DSNU/PRNU mode was not working.
* Fixed the bug to set line trigger to off whenever updating the slave trigger parameters
* Fixed the bug in applying digital io user settings for evo
* Fixed the bug in initializing the device voltage selector correctly
* Improvements on reset level control
  * Increased the reset level settle time
  * Improved reset level offset calibration by using float divider.
* Fixed the salt and pepper bug


## Incompatibilities

* Removed the truncation support of the gain control region
* The gain control region width and offset is limited to certain multiples of an internal constant.
  * Therefore the offsetX and Width of the gain control region may not be as precise as before.
  * If the gain control is outside an ROI the start of the ROI should be precise.
  * For more information like inaccuracies check the feature reference.
* The each line info block size has been reduced.
  * Unused parts were removed.
* Black level is not compatible anymore because sensor timings have changed


## Errata


* The Internal DSNU/PRNU creation may not work properly. Please check the result is good or not.
* In Master Slave Mode there may be a constant shift between the cameras
* The gain control is not working when gain control region is outside the ROI
* The pixels 10 and 11 contain wrong data when enabling the each line info block.
  * In future those pixels should contain image data


## Docs

* Adapted the description of LineStatus in Each Line Info Block
* Added new device status code and error codes
* Adapted the notes for the gain control region offset X and width regarding the precision
* Added MultiRegionMerge feature and updated RegionSelector enum entries
* Adapted the description of Flat Field Correction Calibration Mode
* Replaced in many places the text:
  * **It will be removed from package 3.0.0**
  * By a text without version information.
* Adapted Feature Availability for Multi ROI and removed ax_dsxge.